TM4C Series Product Line

The TM4C MCU family provide a broad portfolio of highly connected 32-bit ARM® Cortex™-M4F microcontrollers with integrated communication peripherals such as CAN, USB, and Ethernet. TM4C MCU’s offer clock speeds from 80 to 120 MHz, scalable flash options from 32 kB up to 1 MB, and come in a variety of package/pin count combinations. A detailed breakdown of the TM4C123x and TM4C129x families with a full listing of products is provided in our Product Selector Guide. All TM4C MCUs are supported by the TivaWare™ for C Series software development kit which allows customers to get started quickly, write production-ready code easily, and minimize their overall cost of software ownership. The software kit provides libraries for each device peripheral with TI-developed, tested, and maintained API's. A variety of examples are offered leveraging TI development kits such as the EK-TM4C123GXL LaunchPad and the EK-TM4C1294XL LaunchPad and these example projects offer a starting point for new development as well as an introduction on how to leverage TivaWare API’s for device peripherals.