                                                                   Jan 2, 2008
 TEXAS INSTRUMENTS
   3535 40th Ave. NW, Suite 103
   ValleyHigh Business Center
   ROCHESTER, MN 55901
   PHONE 507-536-2901  Brian Ashelin(ext.108) 
   FAX  507-536-2922

   Texas Instruments	
   PART NO. Wireless 2Way
   REV. C

  
 THIS ARCHIVED (WINZIP) FILE "Wireless 2Way.ZIP" CONTAINS 24 FILES.

   Wireless 2Way.GTO = TOP SILKSCREEN GERBER FILE
   Wireless 2Way.GTS = TOP SOLDER MASK GERBER FILE
   Wireless 2Way.GTL = LAYER 1 TOP SIGNAL GERBER FILE
   Wireless 2Way.GP1 = LAYER 2 INTERNAL GROUND PLANE GERBER FILE
   Wireless 2Way.GP2 = LAYER 3 INTERNAL POWER PLANE GERBER FILE
   Wireless 2Way.GBL = LAYER 4 BOTTOM SIGNAL GERBER FILE
   Wireless 2Way.GBS = BOTTOM SOLDER MASK GERBER FILE
   Wireless 2Way.GBO = BOTTOM SILKSCREEN GERBER FILE
   Wireless 2Way.GTP = TOP PASTE STENCIL GERBER FILE
   Wireless 2Way.GBP = BOTTOM PASTE STENCIL GERBER FILE
   Wireless 2Way.GG1 = DRILL GUIDE GERBER FILE
   Wireless 2Way.GD1 = DRILL DRAWIING GERBER FILE
   Wireless 2Way.GM3 = FAB DIMENSION GERBER FILE
   Wireless 2Way.GM1 = TOP ASSEMBLY DRAWING GERBER FILE
   Wireless 2Way.GM5 = BOTTOM ASSEMBLY DRAWING GERBER FILE
   Wireless 2Way.DRR = ASCII DRILL SIZE REPORT
   Wireless 2Way.TXT = ASCII DRILL FILE
   Wireless 2Way.DRL = BINARY DRILL FILE
   Wireless 2Way.APR = APERTURE FILE
   README.TXT = THIS FILE
   FAB NOTES.DOC = FAB NOTES DOCUMENT
   PICK PLACE FOR Wireless 2Way.XLS = PICK AND PLACE SPREADSHEET
   Wireless 2Way RevC BOM.XLS = BILL OF MATERIALS
   Wireless 2Way ASCII.PCB = BOARD DESIGN IN PROTEL PCB V2.8 ASCII FORMAT
 
  

   Any Questions? ... Please call ?






READ.ME
