DRC Rules Export File for PCB: D:\TIDA-00289\Completed_E3\Design Files_TIDA-00289\TIDA-00289.PcbDoc
RuleKind=Clearance|RuleName=Less Than 9 mils from PAD to PAD|Scope=Board|Minimum=7.00
RuleKind=Clearance|RuleName=Poly_Poly|Scope=Board|Minimum=15.00
RuleKind=Clearance|RuleName=Clearance|Scope=Board|Minimum=8.00
RuleKind=Width|RuleName=Width|Scope=Board|Minimum=8.00
RuleKind=SolderMaskExpansion|RuleName=SolderMaskExpansion|Scope=Board|Minimum=2.50
RuleKind=ShortCircuit|RuleName=ShortCircuit|Scope=Board|Allowed=0
RuleKind=MinimumAnnularRing|RuleName=MinimumAnnularRing_ThermalPadVias|Scope=Board|Minimum=5.91
RuleKind=MinimumAnnularRing|RuleName=MinimumAnnularRing|Scope=Board|Minimum=5.91
RuleKind=Clearance|RuleName=Via to Via|Scope=Board|Minimum=8.00
RuleKind=Clearance|RuleName=SMT Pin Via|Scope=Board|Minimum=8.00
RuleKind=Clearance|RuleName=Poly_ All|Scope=Board|Minimum=12.00
