Removed Pin From Net: NetName=FAULT_IND Pin=C6-1
Removed Pin From Net: NetName=GND Pin=C6-2
Removed Pin From Net: NetName=FAULT_IND Pin=Q2-1
Removed Pin From Net: NetName=NetC7_1 Pin=Q2-2
Removed Pin From Net: NetName=GND Pin=Q2-3
Removed Pin From Net: NetName=NetC7_1 Pin=R20-2
Removed Pin From Net: NetName=GND Pin=R24-1
Removed Member From Class: ClassName=Pg2-Main Member=C6
Change Component DesignItemId : Designator=Q2 Old DesignItemId=BC857C-7-F, Diodes Inc. New DesignItemId=TR-BC850
Change Component Comment : Designator=Q2 Old Comment=BC857C-7-F New Comment=TR-BC850
Change Component Description : Designator=Q2 Old Description=Transistor, PNP, 45V, 0.1A, SOT-23 New Description=Transistor, N-Chan GP, 45V, 100mA
Change Component Library : Designator=Q2 Old Library=Bipolar_Transistor.IntLib New Library=PADSlegacy_Active.IntLib
Added Component: Designator=Q4(SOT-23)
Added Pin To Net: NetName=GND Pin=Q2-2
Added Pin To Net: NetName=GND Pin=Q4-2
Added Pin To Net: NetName=NetC7_1 Pin=Q4-3
Added Pin To Net: NetName=NetQ2_1 Pin=Q2-1
Added Pin To Net: NetName=NetQ2_1 Pin=R24-1
Added Net: Name=NetQ2_1
Added Pin To Net: NetName=NetQ2_3 Pin=Q2-3
Added Pin To Net: NetName=NetQ2_3 Pin=Q4-1
Added Pin To Net: NetName=NetQ2_3 Pin=R20-2
Added Net: Name=NetQ2_3
Added Member To Class: ClassName=Pg2-Main Member=Component Q4 TR-BC850
