Reporting Options

# File in Newer Format

Date | : | 11/25/2014
Time | : | 10:03:33 AM
Filename | : | \\dataserver\pcb\PCB-BLR\TEMPORARY WORKS\Sharanu\TIDA-00199\NOV_25_2014\Isolated IGBT Gate-Drive Fly-buck™ Power Supply with 8 Outputs\TIDA-00199_revB.PcbDoc

Version | Warning
--- | ---
Release 10 update 1 | CAUTION - New Clearance Rule subscopes targeting differential pairs were introduced. Be aware that your design might contain Clearance Rules using those subscopes that cannot be read in previous versions.
Release 10 update 15 | CAUTION - Support of Solder Mask and Paste Mask expansions for Tracks, Arcs, Fills and Regions was introduced. Be aware that your design might contain Solder Mask and Paste Mask expansions for these types of primitives that cannot be read in the version of Altium Designer you are currently using.
Altium Designer update 19 | CAUTION - Air Gap Width attribute was introduced to Polygon Connect Style Rule. Be aware that your design might contain Polygon Connect Style Rules with new Air Gap Width attribute cannot be read in the version of Altium Designer you are currently using.
Release 13 | CAUTION - Silk To Solder Mask Clearance Rules are converted to Silkscreen Over Component Pads Rules.
Release 14 | CAUTION - The Differential Pairs Routing rule added support for control of the width. Be aware that these widths must be manually entered as Width rules in this version.

This file was generated by a later version of the software