Design Name C:/userdata/Boards/ADS3XRFXX_E/ADC3XRFXXEVM_E.brd
Date Thu Aug 18 11:14:22 2016
Drawing Statistics:
Drawing Extents XL(-10651.00) YL(-11685.00) XU(37349.00) YU(24315.00)
Dimensions in mils with 2 decimal places
Package Symbols: Total(382) Mirrored(170) Embedded(0) Pins(1528)
Mechanical Symbols: Total(4) Mirrored(1) Pins(0)
Format Symbols: Total(7)
DRC State: UP TO DATE
DRC Errors: 0
Short DRC: 0
Waived DRC: 47
Padstack Definitions: 237
Dynamic shapes: Total(70) Out_of_date(0)
Functions: Assigned(386) Unassigned(0) Total(386)

Connection Statistics:
Connections: W/Rats(1004) No/Rats(0) Total(1004)
Already Connected: W/Rats(1004) No/Rats(0) Total(1004)
Missing Connections: W/Rats(0) No/Rats(0) Total(0)
Dangling Connections (See logfile): 1
Connection Completion: W/Rats(100.00%) No/Rats(0.00%) Total(100.00%)
Manh Distance (inches): 285.87
Etch Length (inches): W/Rats(324.49) No/Rats(0.00) Total(324.49)
Number of Vias: W/Rats(2983) No/Rats(0) Total(2983)
Vias per Connection: W/Rats(2.97) No/Rats(0.00)Total(2.97)
SMD pins with attached clines: 592

Layout Statistics:
Components: Placed(382) Unplaced(0) Total(382)
Nets: W/Rats(235) No/Rats(0) Total(235)
Pins: W/Rats(1239) No/Rats(0) Unused(283) Unplaced(0) Total(1522)
Equivalent ICs (1 pin = 1/14 EIC): 108
RatTs: 0
Router Keepin (in): (0.0000,0.0000) by (0.0000,0.0000)
Layout area (sq in): 0.00
Average ratlength (in): 0.3
Rat density (in/sq in): 0.000
Double-sided rat density (in/sq in): 0.000

Layout/Pin Density Statistics
Layer | Layout Area (sq in) | Components | Pins | Layout Density (sq in/EIC) | Pin Density (pins/sq in)
External(Double-Sided) | 0.00 | 382 | 1528 | 0.000 | 0.000
Embedded(0) | 0.00 | 0 | 0 | 0.000 | 0.000
Design | 0.00 | 382 | 1528 | 0.000 | 0.000

Etch Layer Statistics:

Layer | Clines/Carcs | Shapes(voids) | Rectangles | Lines/Arcs | Text | Components(Pins)
TOP | 646 | 49(278) | 0 | 0 | 1 | 212(543)
L2_GND | 206 | 1(509) | 0 | 0 | 1 | 0(0)
L3_PWR | 163 | 5(982) | 0 | 0 | 1 | 0(0)
L4_SIG | 248 | 29(342) | 0 | 0 | 1 | 0(0)
L5_GND | 206 | 1(509) | 0 | 0 | 1 | 0(0)
L6_PWR | 187 | 6(1024) | 0 | 0 | 1 | 0(0)
L7_GND | 206 | 1(509) | 0 | 0 | 1 | 0(0)
BOTTOM | 638 | 28(353) | 0 | 0 | 1 | 170(985)